|  |  |  |
| --- | --- | --- |
| **Pollutant** | **Averaging Time** | **Level** |
| [Carbon Monoxide (CO)](https://www.epa.gov/co-pollution/timeline-carbon-monoxide-co-national-ambient-air-quality-standards-naaqs) | Maximum eight hour daily mean | 10mg/m3 |
| **Sulphur dioxide** | One hour  One day | 350 μg/m3 not to be exceeded more than 24 times a calendar year  125 μg/m3 not to be exceeded more than 3 times a calendar year |
| **Nitrogen dioxide** | One hour  Calendar year | 200 μg/m3not to be exceeded more than 18 times a calendar year  40 μg/m3 |
| **PM10** | One day  Calendar year | 50 µg/m3, not to be exceeded more than 35 times a calendar year  40 µg/m3 |
| **PM2.5** | Calendar year | 25 μg/m3 |